[Contents] [Prev] [Next] [Index] [Report an Error]

# Stopping the SRC Software

To gracefully shut down the SRC software and power off the system, in operational mode, enter the following command:

`

user@host> request system halt

`

This command stops all system components, halts the operating system, and powers down the C Series Controller.

| Note: The request system halt command does not give you the opportunity to restart the system from the CLI.

For example:

    user@host> request system halt
    Halt the system [yes,no] ? (no) y
    BroadcaStopping HAL daemon: [  OK  ]
    Stopping system message bus: [  OK  ]
    Stopping atd: [  OK  ]
    Shutting down xfs: [  OK  ]
    Stopping sshd:[  OK  ]
    Shutting down smartd: [  OK  ]
    Stopping snmpd: [  OK  ]
    Stopping xinetd: [  OK  ]
    Stopping acpi daemon: [  OK  ]
    Stopping crond: [  OK  ]
    Stopping autofs:  [  OK  ]
    Stopping nscd: [  OK  ]
    Shutting down ntpd: [  OK  ]
    Stopping NFS statd: [  OK  ]
    Stopping irqbalance: [  OK  ]
    Stopping portmap: [  OK  ]
    Shutting down kernel logger: [  OK  ]
    Shutting down system logger: [  OK  ]
    Stopping pcmcia:  unloading Kernel Card Services
    [  OK  ]
    Stopping sysstat:  [  OK  ]
    Starting killall:  [  OK  ]
    Sending all processes the TERM signal...
    Sending all processes the KILL signal...
    Saving random seed:
    Syncing hardware clock to system time
    Turning off swap:
    Turning off quotas:
    Unmounting pipe file systems:
    Unmounting file systems:
    Halting system...
    md: stopping all md devices.
    md: md0 switched to read-only mode.
    Synchronizing SCSI cache for disk sda:
    Power down.
    acpi_power_off called

#### Related Topics

- Restarting an SRC Module or Component
- Rebooting the SRC Software

[Contents] [Prev] [Next] [Index] [Report an Error]