[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring an SAE Group

Use the shared option of the set slot number sae shared command to add a new group. Use the shared sae group name command to configure the group.

To configure a group:

1. From configuration mode, add a group. For example, to add a group called REGION-1 in the path /SAE/:
   `
   [edit]
   user@host# set slot 0 sae shared /SAE/REGION-1
   `
2. Commit the configuration.
   `
   [edit]
   user@host# commit
   commit complete.
   `
3. Configure the group as you would a shared SAE configuration.

       [edit]
       user@host# edit shared sae group REGION-1 ?
       Possible completions:
         <[Enter]>           Execute this command
       > configuration
       > dhcp-classifier Configure a DHCP classification script
       > group               Group of SAE configuration properties
       > user-classifier Configure a subscriber classification script
         |                    Pipe through a command

#### Related Topics

- Configuring an SAE Group with the C-Web Interface
- Creating Grouped Configurations for the SAE (SRC CLI)
- Initially Configuring the SAE
- Deleting Default Configurations Within an SAE Group
- Configuring Local Properties for the SAE (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]