[Contents] [Prev] [Next] [Index] [Report an Error]

# Limiting Subscribers on Router Interfaces (C-Web Interface)

You can limit the number of authenticated subscribers who connect to an IP interface on the router. This plug-in does not limit the number of unauthenticated subscribers who connect to an IP interface, and does not limit the number of subscribers who connect to a physical or link-layer interface. In the case of subscriber interfaces, the plug-in limits the number of authenticated subscribers on the subscriber interface but not on the underlying primary IP interface.

To set up a plug-in that limits the number of subscribers on interfaces:

1. Click Configure, expand Shared>SAE, and then expand the SAE group for which you want to configure subscriber limits.
2. In the side pane, expand Configuration>Plug Ins.
3. Expand the plug-in that you created for limiting subscribers, and then click Interface Subscriber Limit.

   The Interface Subscriber Limit pane appears.

4. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

[Contents] [Prev] [Next] [Index] [Report an Error]