[Contents] [Prev] [Next] [Index] [Report an Error]

# Specifying Policy Server Identifiers in Messages

Use the following configuration statements to configure policy server identifiers for the JPS:

`

slot number jps {
  policy-server-id policy-server-id;
  use-psid-in-gate-commands;
}

`

To configure policy server identifiers for the JPS:

1. From configuration mode, access the configuration statement that configures the policy server identifiers.
   `
   user@host# edit slot 0 jps
   `
2. (Optional) Specify the policy server identifier so that the JPS can be identified in messages sent to CMTS devices.
   `
   [edit slot 0 jps]
   user@host# set policy-server-id policy-server-id
   `
3. (Optional) Configure the JPS so that the policy server identifier is specified in messages sent to the RKS.
   `
   [edit slot 0 jps]
   user@host# set use-psid-in-gate-commands
   `

   When the JPS is communicating only with PCMM I03 CMTS devices, the value must be true. When the JPS is communicating with any pre-PCMM I03 CMTS devices, the value must be false.

4. (Optional) Verify your configuration.

       [edit slot 0 jps]
       user@host# show

#### Related Topics

- Modifying the JPS Configuration (C-Web Interface)
- Specifying Application Manager Identifiers for Policy Servers
- Adding Objects for Policy Servers to the Directory
- Modifying the JPS Configuration
- Viewing Server Process Information

[Contents] [Prev] [Next] [Index] [Report an Error]