[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the Local Diameter Peer (SRC CLI)

Use the following configuration statements to configure the local Diameter peer:

`

slot number ims aracf-rq {
  protocol protocol;
  port port;
  address address;
  origin-host origin-host;
  origin-realm origin-realm;
}

`

To configure the local Diameter peer:

1. From configuration mode, access the statement that configures the Diameter peer.
   `
   user@host# edit slot 0 ims aracf-rq
   `
2. (Optional) Specify the protocol used for the transport layer.
   `
   [edit slot 0 ims aracf-rq]
   user@host# set protocol protocol
   `
3. (Optional) Specify the port used for incoming connections.
   `
   [edit slot 0 ims aracf-rq]
   user@host# set port port
   `
4. (Optional) Specify the IP address of the local peer.
   `
   [edit slot 0 ims aracf-rq]
   user@host# set address address
   `
5. (Optional) Specify the Diameter identifier for the local endpoint that is the originator of the Diameter message.
   `
   [edit slot 0 ims aracf-rq]
   user@host# set origin-host origin-host
   `
6. (Optional) Specify the Diameter identifier for the realm of the local endpoint that is the originator of the Diameter message.
   `
   [edit slot 0 ims aracf-rq]
   user@host# set origin-realm origin-realm
   `
7. (Optional) Verify your configuration.

       [edit slot 0 ims aracf-rq]
       user@host# show
       protocol tcp;
       port 3868;
       address 127.0.0.1;
       origin-host testserver;
       origin-realm testrealm;
       peer 1 {
         address 127.0.0.1;
         origin-host testclient;
       }

#### Related Topics

- Overview of an IMS Environment
- Configuring the IMS Software (SRC CLI)
- Configuring the Remote Diameter Peer (SRC CLI)
- Monitoring IMS (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]