[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Gigabit Ethernet Interfaces for IPv6 (C-Web Interface)

To allow remote access to the C Series Controller, you configure the Gigabit Ethernet interfaces. You can specify an IP address with mask for an interface.

To configure a Gigabit Ethernet interface for IPv6:

1. Click Configure>Interfaces.

   The Interfaces pane appears.

2. Create an interface from the Create new list.
   - To create a new interface, select Interface. In the dialog box, type a name for the new interface, and click OK.
   - To create an eth1, eth2, or eth3 interface, select eth1, eth2, or eth3, and click OK.
3. To specify the unit:
   1. From the Create new list, select Unit.
   2. In the dialog box, type a number for the new unit, and click OK.
4. To specify an IPv6 address for the new unit, expand Unit: < number >, and expand Family in the side pane.
   1. In the side pane, click Inet6.

      The Interfaces pane appears.

   2. From the Create new list, select Address.
   3. In the dialog box, type a name for the new address, and click OK.

#### Related Topics

- Configuring Loopback Interfaces for IPv4 (C-Web Interface)
- Configuring Loopback Interfaces for IPv6 (C-Web Interface)
- Configuring Gigabit Ethernet Interfaces for IPv4 (C-Web Interface)
- Configuring Tunnel Interfaces (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]