[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Information About SAE Device Drivers with the CLI

#### Purpose

View information about SAE device drivers. Each device driver manages one logical router instance.

#### Action

To view information about the state of SAE device drivers:

`user@host> show sae drivers`

    JUNOSe Driver
    Device name                           default@dryad
    Device type                           junose
    Device IP                             10.227.7.244
    Local IP                              10.227.7.172
    TransportRouter                       default@dryad
    Device version                        7.2.0
    Start time                            Tue Feb 13 14:18:44 EST 2007
    Number of notifications               20
    Number of processed added             14
    Number of processed changed           0
    Number of processed deleted           6
    Number of provisioning attempt        30
    Number of provisioning attempt failed 0
    Number of outstanding decisions       0
    Number of SAP                         7
    Number of PAP                         1
      Job Queue
      Size                  0
      Age (ms)              1
      Total enqueued        28
      Total dequeued        28
      Average job time (ms) 426
      State Synchronization
      Number recovered subscriber sessions              0
      Number recovered service sessions                 0
      Number recovered interface sessions               0
      Number invalid subscriber sessions                0
      Number invalid service sessions                   0
      Number invalid interface sessions                 0
      Background restoration start time                 Tue Feb 13 14:18:49 EST 2007
      Background restoration end time                   Tue Feb 13 14:18:49 EST 2007
      Number subscriber sessions restored in background 0
      Number of provisioning objects left to collect    0
      Total number of provisioning objects to collect   11
      Start time                                        Tue Feb 13 14:18:45 EST 2007
      End time                                          Tue Feb 13 14:18:47 EST 2007
      Number of synched contexts                        7
      Number of post-sync jobs                          6

To view information about the state of a particular device driver, specify all or part of the virtual router name. For JUNOS router drivers and PCMM drivers, use the format default@routerName.

`user@host> show sae drivers device-name device-name`
`

`

To view only the virtual router names for the device driver:

`user@host> show sae drivers brief`

    Router Drivers
    Router Name              Router Type
    default@simJunos            junos

To restrict the number of displayed results:

`user@host> show sae drivers maximum-results maximum-results`
`

`

#### Related Topics

- Initially Configuring the SAE
- Shutting Down the Device Drivers
- Viewing Information About Device Drivers
- Viewing Statistics for Device Drivers with the CLI

[Contents] [Prev] [Next] [Index] [Report an Error]