> - Downloads
> - Example: Managing Specific Interfaces
> - Related Topics
> - Overview of Configuring Classification Scripts
> - Overview of Classification Scripts
> - Sending DHCP Options to the JUNOSe Router
> - DHCP Options Supported on the SAE

> ## Example: Managing Specific Interfaces

> This example causes the SAE to load the DHCP policy group on IP interfaces on Fast Ethernet modules in slot 3/port 1, slot 1/port 1, or any port on slot 2. The SAE then manages these interfaces.

>     [edit shared network device erx-node2 interface-classifier rule rule-1]
>     user@host# show
>     target /junose/DHCP;
>     condition {
>       interfaceName=FastEthernet3/1;
>       interfaceName=FastEthernet1/1;
>       interfaceName=FastEthernet2/*;
>     }

> #### Published: 2009-09-13

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.

Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.