[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring TLS on the SAE

Use the following configuration statements to configure TLS on the SAE:

`

shared sae configuration driver junos security {
  need-client-authentication;
  certificate-identifier private-key;
}

`

To configure TLS on the SAE:

1. From configuration mode, access the configuration statement that configures security for the JUNOS TLS connection. In this sample procedure, the JUNOS driver is configured in the west-region group.
   `
   user@host# edit shared sae group west-region configuration driver junos security
   `
2. (Optional) Specify whether or not the SAE requests a client certificate from the router when a connection to the router is established.
   `
   [edit shared sae group west-region configuration driver junos security]
   user@host# set need-client-authentication
   `
3. Specify the name of certificate to be used for TLS communications.
   `
   [edit shared sae group west-region configuration driver junos security]
   user@host# set certificate-identifier private-key
   `
4. (Optional) Verify your TLS configuration.

       [edit shared sae group west-region configuration driver junos security]
       user@host# show
       need-client-authentication;
       certificate-identifier privatekey;

#### Related Topics

- Configuring TLS on the SAE
- Configuring the SAE to Use TLS
- Configuring the SAE to Manage JUNOS Routing Platforms
- Monitoring Interactions Between the SAE and JUNOS Routing Platforms
- BEEP Connection Between JUNOS Routing Platforms and the SAE

[Contents] [Prev] [Next] [Index] [Report an Error]