> - Downloads
> - Configuring DOCSIS Actions (C-Web Interface)
> - Related Topics
> - Delivering QoS Services in a Cable Environment
> - Configuring DOCSIS Actions (SRC CLI)

> # Configuring DOCSIS Actions (C-Web Interface)

> You can configure Data over Cable Service Interface Specifications (DOCSIS) actions for PacketCable Multimedia Specification (PCMM) policy rules.

> The types of DOCSIS actions that you can create are:

> - Best effort
> - Downstream
> - Non-real-time polling service
> - Real-time polling service
> - Unsolicited grant service
> - Unsolicited grant service with activity detection
> - Parameter—This is a DOCSIS action with the service flow scheduling type set to a trafficProfileType parameter. You must enter a trafficProfileType parameter that has been created and committed.

> To configure a DOCSIS action:

> 1. In the side pane, select a PCMM policy rule.
> 2. From the Create new list, select the type of DOCSIS action that you want to create. Type a name for the action, and click OK.
> 3. Enter information as described in the Help text in the main pane, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.