[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Resolution Information for a NIC Proxy (SRC CLI)

Use the following statements to configure resolution information for a NIC proxy:

`

nic-proxy-configuration name resolution {
  resolver-name resolver-name;
  key-type key-type;
  value-typevalue-type;
  expect-multiple-values;
  constraints constraints;
}

`

To configure resolution information for a NIC proxy:

1. From configuration mode, access the configuration statement that specifies the NIC proxy configuration.
   `
   [edit]
   user@host# component-hierarchy nic-proxy-configuration name resolution
   `

   For example:

   `
   [edit]
   user@host# edit shared sae configuration nic-proxy-configuration ip resolution
   `
2. Specify the NIC resolver that this NIC proxy uses.
   `
   [edit shared sae configuration nic-proxy-configuration ip resolution]
   user@host# set resolver-name resolver-name
   `

   This resolver must be the same as one that is configured on the NIC host. For example:

   `
   [edit shared sae configuration nic-proxy-configuration ip resolution]
   user@host# set resolver-name /realms/ip/A1
   `
3. Specify the NIC data type that the key provides for the NIC resolution.
   `
   [edit shared sae configuration nic-proxy-configuration ip resolution]
   user@host# set key-type key-type
   `

   For example:

   `
   [edit shared sae configuration nic-proxy-configuration ip resolution]
   user@host# set key-type ip
   `

   To qualify data types, enter a qualifier within parentheses after the data type; for example, to specify username as a qualifier for the key LoginName:

   `
   [edit shared sae configuration nic-proxy-configuration ip resolution]
   user@host# set key-type LoginName (username)
   `
4. Specify the type of value to be returned in the resolution for the application that uses the NIC proxy.
   `
   [edit shared sae configuration nic-proxy-configuration ip resolution]
   user@host# set value-type value-type
   `

   For example:

   `
   [edit shared sae configuration nic-proxy-configuration ip resolution]
   user@host# set value-type SaeId
   `
5. (Optional) If the key can have more than one value, specify that the key can have multiple corresponding values.
   `
   [edit shared sae configuration nic-proxy-configuration ip resolution]
   user@host# set expect-multiple-values
   `
6. (Optional. Available at the Advanced editing level.) If the application provides a constraint in the resolution request, specify the data type for the constraint. The constraint represents a condition that must or may be satisfied before the next stage of the resolution process can proceed.
   `
   [edit shared sae configuration nic-proxy-configuration ip resolution]
   user@host# set constraints constraints
   `

#### Related Topics

- Before You Configure a NIC Proxy
- Changing the Configuration for the NIC Proxy Cache (SRC CLI)
- Configuring a NIC Proxy for NIC Replication (SRC CLI)
- Configuration Statements for NIC Proxies
- Overview of NIC Proxy Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]