[Contents] [Prev] [Next] [Index] [Report an Error]

# Safety Notices

For your safety, before installing the system, review all safety notices in this topic.

## Lithium Battery

| Warning: There is a danger of explosion if the battery is incorrectly replaced. Return the device to the manufacturer for battery replacement. Moreover, never open the chassis under any circumstances. Doing so will also void the warranty.

| Warning: La batterie présente un risque d’explosion si elle n’est pas remplacée comme il se doit. Retournez l’appareil au fabricant pour faire remplacer la batterie. Le châssis ne doit par ailleurs en aucun cas être ouvert. Cela annulerait la garantie.

## Power Disconnection

| Warning: Before working on a device that has an On/Off switch, turn the power off and disconnect the power cord to all power supplies. For DC power supplies, locate the circuit breaker on the panel board that services the DC circuit, switch the circuit breaker to the off position, and tape the switch handle of the circuit breaker in the off position.

| Warning: Avant de commencer à travailler sur un appareil muni d’un interrupteur On. Off (Marche/Arrêt), Coupez l’alimentation et débranchez le cordon d’alimentation de toute source d’alimentation. Dans le cas d’une alimentation à courant continu, repérez le disjoncteur sur le tableau de contrôle qui alimente le circuit c.c., placez-le en position d’off (arrêt) et maintenez le bouton du disjoncteur en position d’arrêt à l’aide de ruban adhésif.

## Power Cable Warning

| Warning: This unit has two power cables. To avoid electric shock, disconnect both power cables before servicing the unit.

| Warning: Cette unité possède deux cordons d’alimentation. Pour supprimer tout risque électrique, débranchez les deux cordons d’alimentation de l’unité.

## Power Cable Warning (Japanese)

| Warning: The attached power cable is only for this product. Do not use the cable for another product.

## Working with Lasers

Some Juniper Networks devices are equipped with fiber-optic ports, which emit radiation that may be harmful to the human eye. Fiber-optic ports are considered Class 1 laser or Class 1 LED ports.

| Warning: Class 1 Laser product.

| Warning: Class 1 LED product.

| Warning: Do not stare into the laser beam or view it directly with optical instruments.

To avoid exposure to radiation, do not stare into the aperture of a fiber-optic port. Invisible radiation might be emitted from the aperture of the port when no fiber cable is connected.

These products have been tested and found to comply with Class 1 limits of IEC 60825-1, IEC 60825-2, EN 60825-1, EN 60825-2, and 21CFR1040.

## VCCI Compliance

| Warning: This is a Class A product. In a domestic environment this product may cause radio interference, in which case the user may be required to take adequate measures. (VCCI-A)

[Contents] [Prev] [Next] [Index] [Report an Error]