[Contents] [Prev] [Next] [Index] [Report an Error]

## Event Traps

Table 18 lists the event traps.

Table 18: Event Traps

Trap Event | Trap ID | Text Displayed
--- | --- | ---
saeLicenseNetworkCapacity | 9 | $S:SAE:The total number of sum-weighted line cards allocated in this SRC network is $LINE_CARD_NUMBER ($THRESHOLD_PERCENTAGE)%. This $L the network ERX capacity threshold of $T sum-weighted line cards.: $A
saeServiceSessionLicense | 11 | $S:LICENSE SERVER:$SERVICE_SESSIONS ($SERVICES_PERCENTAGE%) of the available licensed service sessions are in use.: $A
routerConnClosed | 211 | When juniSaeRouterUseFailOver is FALSE: INFORMATION:SAE Router Driver: The router connection to $juniSaeRouterClientId has been closed.:RAISE When juniSaeRouterUseFailOver is TRUE: INFORMATION:SAE Router Driver:The router connection to $juniSaeRouterClientId has been closed and redirected to $juniSaeRouterFailOverIp:$juniSaeRouterFailOverPort:RAISE
routerConnDown | 212 | INFORMATION:SAE Router Driver:The router connection to $juniSaeRouterClientId went down.:RAISE
routerConnRejected | 213 | INFORMATION:SAE Router Driver:The router connection from $juniSaeRouterClientId has been rejected.:RAISE
routerConnUp | 210 | INFORMATION:SAE Router Driver:A new router connection was established with $juniSaeRouterClientId.:RAISE
routerConfOutOfSynch | 214 | When the trap is raised, the text displayed is: INFORMATION:SAE Router Driver: The configured state of router $juniSaeRouterClientId is out of synch with SAE. The configured action to be taken by SAE is $configuredAction.:RAISE When the trap is cleared, the text displayed is: INFORMATION:SAE Router Driver: The configured state of router $juniSaeRouterClientId is successfully resynchronized with SAE.:CLEAR
agentStarted | 110 | INFORMATION:Agent: The agent has started.:RAISE
agentRestartFailed | 111 | CRITICAL: Agent: The agent has failed to restart after $ATTEMPTS attempts:RAISE
agentShutdown | 112 | INFORMATION:Agent:The agent has shutdown.:RAISE
componentUp | 114 | INFORMATION:$I: This component is up.:RAISE
componentDown | 115 | INFORMATION:$I: This component is down:RAISE
dirConnected | 130 | INFORMATION:$I:The directory connection has been established with $LDAP_HOST on port $LDAP_PORT, and has a type of $CONNECTION_TYPE.:RAISE
dirConnectionFailure | 131 | CRITICAL:$I:The directory connection with $LDAP_HOST has failed.:RAISE
dirNotAvail | 132 | CRITICAL:$I:A directory connection is not available.:RAISE
nicHostRedundStateSwitched | 240 | INFORMATION:NIC Host: The redundancy state of the NIC Host has switched to $juniNicHostRedundState.:RAISE
nicHostMisconfigured | 241 | INFORMATION:NIC Host: The NIC Host failed to start due to misconfiguration. The error message is "$MESSAGE".:RAISE
acpSyncCompleted | 290 | INFORMATION: ACP State Sync:ACP finished state sync with SAE for $juniAcpVirtualRouterName.:RAISE
acpRedundStateSwitched | 291 | INFORMATION: ACP Host:The redundancy state of the ACP Host has switched to $juniAcpRedundState.:RAISE
jpsAmConnUp | 260 | INFORMATION: JPS:A new application manager connection was established.:RAISE
jpsAmConnDown | 261 | INFORMATION:JPS:The application manager connection went down.:RAISE
jpsCmtsConnUp | 262 | INFORMATION:JPS:A new CMTS connection was established.:RAISE
jpsCmtsConnDown | 263 | INFORMATION:JPS:A CMTS connection went down.:RAISE
jdbReplicationFailure | 292 | When the trap is raised, the text displayed is: INFORMATION:jdbReplicationFailure:Failed to replicate LDAP data {juniSdxJdbReplicationDirection} neighbor {juniSdxJdbNeighbor}.The latest JDB replicaiton status is:{juniSdxJdbLastStatus }:RAISE When the trap is cleared, the text displayed is: INFORMATION: jdbReplicationFailure:Community directory server {juniSdxJdbNeighbor} latest update status error:CLEAR
systemOperatingFailure | 300 | When the trap is raised, the text displayed is: INFORMATION:System:hardware failure is found with $juniSdxOperatingSensor on system $juniSdxOperatingLocation:RAISE When the trap is cleared, the text displayed is: INFORMATION:System:hardware failure with $juniSdxOperatingSensor on system $juniSdxOperatingLocation is cleared:CLEAR
diskFailure | 301 | When the trap is raised, the text displayed is: INFORMATION:System:disk failure is found:RAISE When the trap is cleared, text displayed is: INFORMATION:System:disk failure is cleared:CLEAR

#### Related Topics

- Overview of SNMP Traps
- Configuring Event Traps
- Alarm State Transitions

[Contents] [Prev] [Next] [Index] [Report an Error]