[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring IMS for Failover (SRC CLI)

Use the following configuration statements to configure IMS for failover:

`

shared ims configuration redundancy {
  state-synchronization;
  state-sync-bulk-size state-sync-bulk-size;
  state-synchronization-timeout state-synchronization-timeout ;
}

`

To configure state synchronization with the SAE:

1. From configuration mode, access the statement that configures redundancy for IMS.
   `
   user@host# edit shared ims configuration redundancy
   `
2. (Optional) Enable state synchronization from the SAE.
   `
   [edit shared ims configuration redundancy]
   user@host# set state-synchronization
   `
3. (Optional) Specify the number of events the SAE sends to IMS at one time during state synchronization.
   `
   [edit shared ims configuration redundancy]
   user@host# set state-sync-bulk-size state-sync-bulk-size
   `
4. (Optional) Specify the time to wait for the first full synchronization request from the SAE after starting or restarting IMS.
   `
   [edit shared ims configuration redundancy]
   user@host# set state-synchronization-timeout state-synchronization-timeout
   `

[Contents] [Prev] [Next] [Index] [Report an Error]