> - Downloads
> - Setting Up SAE Communities (C-Web Interface)
> - Related Topics
> - Setting Up SAE Communities with SRC CLI
> - Using the SAE in a PCMM Environment

> # Setting Up SAE Communities (C-Web Interface)

> You can configure the following for SAE communities:

> - Define the members of an SAE community by adding the IP addresses of SAEs in the community to the virtual router object of the network device in the directory.

>   See Creating Virtual Routers for the CMTS Device (C-Web Interface) .

> - Specify the name of the community manager.

>   See Configuring the SAE to Manage PCMM Devices (C-Web Interface).

> - Configure parameters for the SAE community manager.

>   See Configuring the SAE Community Manager with the C-Web Interface .

> - If there is a firewall in the network, configure the firewall to allow SAE messages through.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.