[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing IPMI Chassis Information

You can view IPMI chassis information for the controller you are currently logged in to and for a remote controller. You must be logged on as a root user.

To display the chassis information on the local controller using IPMI:

1. Log in as root user.
   `
   SRC-PE Release 3.1 [R.3.1.0-12]
   login: root
   `
2. Enter the password.
   `
   Password: password
   `

   You are now logged in as root user.

3. Access the CLI.
   `
   [root@host ~]# cli
   --- SRC CLI 3.1 build CLI.R.3.1.0.012
   (c) 2005-2008 Juniper Networks Inc.
   root@host>
   `
4. Enter the show ipmi chassis command.

   For example:

   `root@host>show ipmi chassis`

       System Power         : on
       Power Overload       : false
       Power Interlock      : inactive
       Main Power Fault     : false
       Power Control Fault  : false
       Power Restore Policy : always-off
       Last Power Event     :
       Chassis Intrusion    : inactive
       Front-Panel Lockout  : inactive
       Drive Fault          : false
       Cooling/Fan Fault    : false

       System Power         : on
       Power Overload       : false
       Power Interlock      : inactive
       Main Power Fault     : false
       Power Control Fault  : false
       Power Restore Policy : always-off
       Last Power Event     :
       Chassis Intrusion    : inactive
       Front-Panel Lockout  : inactive
       Drive Fault          : false
       Cooling/Fan Fault    : false

To display the IPMI chassis information on a remote controller:

1. Log in as root user.
2. Enter the show ipmi host chassis command.
   `
   user@host>show ipmi host host user user chassis
   `
   - host—IP address of remote host IPMI interface
   - user—IPMI username configured in the remote host

   For example:

   `
   root@host>show ipmi host 10.10.10.30 user johndoe chassis
   `

[Contents] [Prev] [Next] [Index] [Report an Error]