[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Dynamic Service Activator (C-Web Interface)

To use Dynamic Service Activator in the SRC network, you configure basic and initial properties, including directory connection and directory eventing properties. You also configure Dynamic Service Activator properties.

For information about these configuration procedures, see:

1. Configuring Local Properties for Dynamic Service Activator (C-Web Interface)
2. Configuring Dynamic Service Activator Properties (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]