> - Downloads
> - Specifying Router Initialization Scripts on the SAE with the CLI
> - Related Topics
> - Accessing the Router CLI
> - Configuring the SAE to Manage JUNOSe Routers with the CLI
> - Monitoring Interactions Between the SAE and the JUNOSe Router
> - Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices

> # Specifying Router Initialization Scripts on the SAE with the CLI

> Use the following configuration statements to specify router initialization scripts for JUNOSe routers:

> `
> shared sae configuration driver scripts {
>   extension-path extension-path ;
>   general general ;
>   junose-pr junose-pr ;
>   junose-xdr junose-xdr ;
> }
> `

> To configure router initialization scripts for JUNOSe routers:

> 1. From configuration mode, access the configuration statements that configure router initialization scripts. In this sample procedure, the scripts are configured in the west-region group.
>    `
>    user@host# edit shared sae group west-region configuration driver scripts
>    `
> 2. Specify the script for JUNOSe routers when the JUNOSe driver uses COPS-PR mode when connecting to the SAE.
>    `
>    [edit shared sae group west-region configuration driver scripts]
>    user@host# set junose-pr junose-pr
>    `
> 3. Specify the script for JUNOSe routers when the JUNOSe driver uses COPS-XDR mode when connecting to the SAE.
>    `
>    [edit shared sae group west-region configuration driver scripts]
>    user@host# set junose-xdr junose-xdr
>    `

>    In COPS-XDR mode, the router does not send the network access server (NAS) IP address to the SAE. If your configuration requires this value, add the following line to a JUNOSe script:

>    `
>    import ERXnasip
>    `
> 4. Configure a router initialization script that can be used for all types of routers that the SRC module supports.
>    `
>    [edit shared sae group west-region configuration driver scripts]
>    user@host# set general general
>    `
> 5. Configure a path to router initialization scripts that are not in the default location, /opt/UMC/sae/lib.
>    `
>    [edit shared sae group west-region configuration driver scripts]
>    user@host# set extension-path extension-path
>    `
> 6. (Optional) Verify your router initialization script configuration.

>        [edit shared sae group west-region configuration driver scripts]
>        user@host# show
>        junose-xdr poolPublisher;

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.