[Contents] [Prev] [Next] [Index] [Report an Error]

## Interface Classification Conditions

Use the fields in this section to define interface classification conditions.

broadcastAddr

- Interface broadcast address.

- Value—Valid broadcast address format

- Example—broadcastAddr.hostAddress=“ 255.255.255.255”

ifAlias

- Description of an interface.

- Value—Interface description that is configured on the router. For JUNOSe routers, it is the description configured with the interface description command.

- Example—ifAlias=“ 1st pppoe int”

ifDesc

- Alternate name of the interface that is used by SNMP. This name is a system-generated name.

- Value
  - On a JUNOSe router, the format of the description is
    `
    ip<slot>/<port>.<subinterface>
    `
  - On the JUNOS routing platform, ifDesc is the same as interfaceName.

- Example—ifDesc=“ IP3/1.1”

interfaceName

- Name of the interface.

- Value
  - Name of the interface in your router CLI syntax
  - FORWARDING_INTERFACE for routing instance (used by traffic mirroring)

- Example—For JUNOSe routers: interfaceName=“ fastethernet6/0.1”

For JUNOS routing platforms: interfaceName=“ fe-0/1/0.0”

For forwarding interface: interfaceName=“ FORWARDING_INTERFACE”

ipAddress

- Interface IP address.

- Value—Valid IPv4 IP address format

- Example—ipAddress=“ 10.10.30.1”

ipMask

- Interface network mask.

- Value—Valid IPv4 IP network mask format

- Example—ipMask=“ 255.255.255.255”

mtu

- Maximum transfer unit configured on the interface.

- Value—32-integer value

- Example—mtu=“ 1492”

nasPortId

- Port identifier of an interface.

- Value—Includes interface name and additional layer 2 information

- Example—nasPortId=“ fastEthernet 3/1” (There is a space between fastEthernet and slot number 3/1 in the nasPortId.)

pppLoginName

- Login name for PPP subscribers.

- Value—Login name in the format username@domain

- Example—pppLoginName=“ pebbles@virneo.net”

radiusClass

- RADIUS class attribute.

- Value—RADIUS class name

- Example—radiusClass=“ Premium”

serviceBundle

- Content of the vendor-specific RADIUS attribute for the service bundle.

- Value—Name of a service bundle

userIpAddress

- Subscriber IP address (PPP only).

- Value—valid IPv4 address

- Example—userIpAddress=“ 192.168.30.15”

virtualRouterName

- Name of the virtual router or routing instance.

- Value—For JUNOSe routers: name of the virtual router in the format vrname@hostname

  For JUNOS routing platforms: name of the routing instance

- Example—virtualRouterName=“ default@erx5”

[Contents] [Prev] [Next] [Index] [Report an Error]