[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Local Properties for the SAE (SRC CLI)

Use the following configuration statements to configure local properties for the SAE:

`

slot number sae {
  base-dn base-dn ;
  real-portal-address real-portal-address ;
  java-runtime-environment java-runtime-environment ;
  java-heap-size java-heap-size ;
  java-new-size java-new-size ;
  java-garbage-collection-options java-garbage-collection-options ;
  port-offset port-offset ;
  snmp-agent;
  shared shared ;
}

`

To configure local properties on the SAE:

1. From configuration mode, access the SAE RADIUS configuration. This configuration is under the slot 0 hierarchy.
   `
   [edit]
   user@host# edit slot 0 sae
   `
2. (Optional) If you store data in the directory in a location other than the default, o=umc, change this value.
   `
   [edit slot 0 sae]
   user@host# set base-dn base-dn
   `
3. Configure the interface on the SAE that the SAE uses to communicate with the router.
   `
   [edit slot 0 sae]
   user@host# set real-portal-address real-portal-address
   `
4. (Optional) If you encounter problems caused by lack of memory, change the maximum memory size available to the JRE.
   `
   [edit slot 0 sae]
   user@host# set java-heap-size java-heap-size
   `
5. Configure the amount of space available to the JRE when the SAE starts.
   `
   [edit slot 0 sae]
   user@host# set java-new-size java-new-size
   `
6. Configure the garbage collection functionality of the Java Virtual Machine.
   `
   [edit slot 0 sae]
   user@host# set java-garbage-collection-options java-garbage-collection-options
   `
7. If you install multiple instances of the SAE on the same host, set a port offset for SAE instances.
   `
   [edit slot 0 sae]
   user@host# set port-offset port-offset
   `
8. (Optional) Enable the SNMP agent to communicate with the SAE.
   `
   [edit slot 0 sae]
   user@host# set snmp-agent
   `
9. (Optional) Configure an SAE group configuration.
   `
   [edit slot 0 sae]
   user@host# set shared shared
   `
10. (Optional) Verify your configuration.

        [edit slot 0 sae]
        user@host# show
        base-dn o=UMC;
        real-portal-address 10.10.4.24;
        java-runtime-environment ../jre/bin/java;
        java-heap-size 896m;
        java-new-size 22m;
        java-garbage-collection-options "-Xbatch -XX:+UseConcMarkSweepGC -XX:CMSInitiatingOccupancyFraction=80 -XX:+UseParNewGC -XX:SurvivorRatio=1 -XX:InitialTenuringThreshold=8 -XX:MaxTenuringThreshold=10 -XX:TargetSurvivorRatio=90 -XX:+UseCMSCompactAtFullCollection -XX:CMSFullGCsBeforeCompaction=0  -XX:+CMSPermGenSweepingEnabled -XX:+CMSClassUnloadingEnabled -XX:+CMSParallelRemarkEnabled";
        port-offset 0;
        snmp-agent;
        shared /SAE/REGION-1;

#### Related Topics

- Configuring Local Properties for the SAE with the C-Web Interface
- Configuring the RADIUS Local IP Address and NAS ID (SRC CLI)
- Configuring an SAE Group
- Initially Configuring the SAE
- Creating Grouped Configurations for the SAE (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]