> - Downloads
> - Verifying the Local Configuration for a Component
> - Related Topics
> - Configuring Basic Local Properties
> - Viewing Information About Components Installed (SRC CLI)
> - Local Properties for SRC Components

> # Verifying the Local Configuration for a Component

> #### Purpose

> Verify the local configuration for a component.

> #### Action

> 1. From configuration mode, access the configuration statement that configures the slot connection. For example, to verify the slot configuration for the NIC:
>    `
>    user@host# edit slot 0 nic
>    `
> 2. Run the show command. For example:

>        [edit slot 0 nic ]
>        user@host# show
>        base-dn o=umc;
>        java-runtime-environment ../jre/bin/java;
>        java-heap-size 128m;
>        snmp-agent;
>        hostname DemoHost;
>        initial {
>          dynamic-dn "ou=dynamicConfiguration, ou=Configuration, o=Management,<base>";
>          directory-connection {
>            url ldap://127.0.0.1:389/;
>            backup-urls ;
>            principal cn=nic,ou=Components,o=Operators,<base>;
>            credentials ********;
>            timeout 10;
>            check-interval 60;
>          }
>          directory-eventing {
>            eventing;
>            signature-dn <base>;
>            polling-interval 15;
>            event-base-dn <base>;
>            dispatcher-pool-size 1;
>          }
>          static-dn "l=OnePop,l=NIC, ou=staticConfiguration, ou=Configuration, o=Management,<base>";
>        }

> #### Published: 2009-09-25

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.