> - Downloads
> - Configuring the JPS
> - Related Topics
> - Overview of the JPS
> - Configuring the JPS (C-Web Interface)
> - Configuring General Properties for the JPS
> - Monitoring the JPS
> - Configuration Statements for the JPS

> # Configuring the JPS

> You can modify the JPS configuration, which includes configuring the logging destinations and connections to the JPS interfaces. Any configuration changes will be applied within 15 seconds.

> Before you configure the JPS, deploy an SRC-managed PCMM network. For more information about PCMM and the SRC software, see Overview of a PCMM Environment.

> You can configure the subscriber configuration, which maps a subscriber address to the CMTS address.

> The tasks to configure the JPS for a cable network environment are:

> - Modifying the JPS Configuration
> - Modifying the Subscriber Configuration

> In addition to configuring the JPS, you might need to perform these tasks:

> - Configuring the SAE to Interact with the JPS
> - Using the NIC Resolver

> #### Published: 2009-09-23

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.