> - Downloads
> - Viewing Statistics for Device Drivers with the CLI
> - Related Topics
> - Shutting Down the Device Drivers (C-Web Interface)
> - Viewing Information About SAE Device Drivers with the CLI
> - Viewing SNMP Information for Routers and Devices with the CLI
> - Viewing Statistics for Specific Device Drivers with the CLI

> # Viewing Statistics for Device Drivers with the CLI

> #### Purpose

> View SNMP statistics for all device drivers.

> #### Action

> `user@host> show sae statistics device common`

>     SNMP Statistics
>     Driver type                    JUNOSE COPS
>     Number of close requests       0
>     Number of connections accepted 0
>     Number of current connections  0
>     Number of open requests        0
>     Server address                 0.0.0.0
>     Server port                    3288
>     Time since last redirect       0

>     SNMP Statistics
>     Driver type                    PACKETCABLE COPS
>     Number of close requests       0
>     Number of connections accepted 0
>     Number of current connections  0
>     Number of open requests        0
>     Server address                 0.0.0.0
>     Server port                    0
>     Time since last redirect       0

>     SNMP Statistics
>     Driver type                    JUNOS
>     Number of close requests       0
>     Number of connections accepted 0
>     Number of current connections  0
>     Number of open requests        0
>     Server address                 0.0.0.0
>     Server port                    3333
>     Time since last redirect       0

> The value of the server address can be either an IPv4 or IPv6 address, depending on the platform.

> #### Published: 2009-09-10

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.