> - Downloads
> - Configuring NIC Test Data (C-Web Interface)
> - Related Topics
> - Configuring NIC Test Data (SRC CLI)
> - Configuring a NIC Proxy (C-Web Interface)
> - Overview of NIC Proxy Configuration

> # Configuring NIC Test Data (C-Web Interface)

> To test a resolution without NIC, you can configure a NIC proxy stub to take the place of the NIC. The NIC proxy stub comprises a set of explicit mappings of data keys and values in the NIC proxy configuration. When the SAE (or another SRC component configured to use a NIC proxy stub) passes a specified key to the NIC proxy stub, the NIC proxy stub returns the corresponding value. When you use a NIC proxy stub, no NIC infrastructure is required.

> For example, you can specify a subscriber’s IP address that is associated with a particular SAE. When the SRC component passes this IP address to the NIC proxy stub, the NIC proxy stub returns the corresponding SAE.

> To use the NIC proxy stub for the SAE:

> 1. Click Configure, and expand Shared>SAE, and then click Configuration.

>    The Configuration pane appears.

> 2. From the Create new list, select NIC Proxy Configuration. Type a name for the new NIC proxy in the dialog box, and click OK.

>    The new NIC proxy configuration appears in the side pane.

> 3. In the side pane, expand the new NIC proxy configuration, and click Test NIC Bindings.

>    The Test NIC Bindings pane appears.

> 4. Click Create, select the Use Test Bindings check box, and then click Apply.
> 5. In the side pane, expand Test NIC Bindings, and click Key Values.
> 6. From the Create new list, select Key Values. Type a name in the dialog box for the key that indicates the NIC data value for the proxy, and click OK.

>    The Key Values name pane appears in the side pane and in the Key Values pane.

> 7. Enter a value for the key that specifies a value for the NIC data type.
> 8. Click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.