> - Downloads
> - Configuring Destination Grouped Networks (SRC CLI)
> - Related Topics
> - Before You Configure Classify-Traffic Conditions
> - Configuring Classify-Traffic Conditions
> - Configuring Destination Networks (SRC CLI)
> - Configuring Destination Grouped Networks (C-Web Interface)

> # Configuring Destination Grouped Networks (SRC CLI)

> You can configure destination networks in grouped format. For JUNOS ASP and JUNOSe IPv6 policy rules, you must enter destination networks in grouped format.

> Use the following configuration statements to add destination networks in a grouped format to a classify-traffic condition:

> `
> policies group name list name rule name traffic-condition name destination-network group-network {
>   network-specifier network-specifier ;
> }
> `

> To add a grouped destination network to a classify-traffic condition:

> 1. From configuration mode, enter the destination network within a classify-traffic condition. For example:
>    `
>    user@host# edit policies group dhcp list in rule forward-dhcp traffic-condition client-dhcp destination-network group-network
>    `
> 2. (Optional) Configure the IP address of the destination network or host.

>    For JUNOS ASP policy rules, you must enter networks in the format <ip address>/<prefix length>.

>    For JUNOSe IPv6 policy rules, you must enter networks in the format <ipv6 address>/<prefix length>.

>    `
>    [edit policies group dhcp list in rule forward-dhcp traffic-condition client-dhcp destination-network group-network]
>    user@host# set network-specifier network-specifier
>    `
> 3. (Optional) Verify your destination network configuration.

>        [edit policies group dhcp list in rule forward-dhcp traffic-condition client-dhcp destination-network group-network]
>        user@host# show
>        network-specifier any;

> #### Published: 2009-09-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.