> - Downloads
> - Specifying a Basic NTP Configuration on a C Series Controller (C-Web Interface)
> - Related Topics
> - Configuring NTP on a C Series Controller

> # Specifying a Basic NTP Configuration on a C Series Controller (C-Web Interface)

> We recommend that you configure NTP on C Series Controllers.

> To configure NTP to operate on a C Series Controller:

> 1. Click Configure, expand System, and then click NTP.

>    The NTP pane appears.

> 2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

>    | Note: If you do not configure a boot server, NTP cannot synchronize with a time server if the server’s time is very far off the local system’s time.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.