> - Downloads
> - Configuring the RADIUS Local IP Address and NAS ID (SRC CLI)
> - Related Topics
> - Configuring the RADIUS Local IP Address and NAS ID with the C-Web Interface
> - Configuring Local Properties for the SAE (SRC CLI)
> - Configuring an SAE Group
> - Initially Configuring the SAE
> - Creating Grouped Configurations for the SAE (SRC CLI)

> # Configuring the RADIUS Local IP Address and NAS ID (SRC CLI)

> Use the following configuration statements to set the local RADIUS address and network access server (NAS ID):

> `
> slot number sae radius {
>   local-address local-address ;
>   local-nas-id local-nas-id ;
> }
> `

> To set the local RADIUS address and NAS ID:

> 1. From configuration mode, access the SAE RADIUS configuration. This configuration is under the slot 0 hierarchy.
>    `
>    [edit]
>    user@host# edit slot 0 sae radius
>    `
> 2. Configure the local IP address that the SAE uses to communicate with RADIUS servers.
>    `
>    [edit slot 0 sae radius]
>    user@host# set local-address local-address
>    `
> 3. Configure the NAS ID that identifies the SAE when it sends RADIUS authentication and accounting records. Typically, the NAS ID is the name of the SAE host.
>    `
>    [edit slot 0 sae radius]
>    user@host# set local-nas-id local-nas-id
>    `
> 4. (Optional) Verify your configuration.

>        [edit slot 0 sae radius]
>        user@host# show
>        local-address 10.10.4.20;
>        local-nas-id SAE.host1;

> #### Published: 2009-09-25

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.