> - Downloads
> - Specifying Router Initialization Scripts on the SAE
> - Related Topics
> - Specifying JUNOS Router Initialization Scripts on the SAE (C-Web Interface)
> - Configuring JUNOS Routing Platforms to Interact with the SAE
> - Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices

> # Specifying Router Initialization Scripts on the SAE

> Use the following configuration statements to specify router initialization scripts for JUNOS routing platforms:

> `
> shared sae configuration driver scripts {
>   extension-path extension-path ;
>   general general ;
>   junos junos ;
> }
> `

> To configure router initialization scripts for JUNOS routing platforms:

> 1. From configuration mode, access the configuration statements that configure router initialization scripts. In this sample procedure, the scripts are configured in the west-region group.
>    `
>    user@host# edit shared sae group west-region configuration driver scripts
>    `
> 2. Specify the router initialization script for JUNOS routing platforms.
>    `
>    [edit shared sae group west-region configuration driver scripts]
>    user@host# set junos junos
>    `
> 3. Configure a router initialization script that can be used for all types of routers that the SRC module supports.
>    `
>    [edit shared sae group west-region configuration driver scripts]
>    user@host# set general general
>    `
> 4. Configure a path to router initialization scripts that are not in the default location, /opt/UMC/sae/lib.
>    `
>    [edit shared sae group west-region configuration driver scripts]
>    user@host# set extension-path extension-path
>    `
> 5. (Optional) From operational mode, verify your router initialization script configuration.

>        [edit shared sae group west-region configuration driver scripts]
>        user@host# show
>        extension-path ;
>        junos iorPublisher;

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.