[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring CMTS-Specific RKS Plug-Ins (C-Web Interface)

You can configure an RKS plug-in for specific CMTS devices. When there are events for the CMTS device, the SAE sends the events to the specified plug-in.

To configure a CMTS-specific RKS plug-in:

1. Click Configure, expand Shared>SAE,>Configuration>Driver, and then click PCCM.

1. Click Configure, expand Shared>SAE, and then expand the SAE group for which you want to create CMTS-specific RKS plug-ins.
2. In the side pane, expand Configuration>Drivers, and then click PCCM.

   The PCMM pane appears.

3. From the Create new list, select CMTS Specific RKS Plug-Ins.
4. Type a name for the new plug-in in the dialog box, and click OK.
5. In the side pane, click the new plug-in.
6. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

#### Related Topics

- Configuring CMTS-Specific RKS Plug-Ins (SRC CLI)
- Adding Objects for CMTS Devices (SRC CLI)
- Creating Virtual Routers for the CMTS Device (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]