[Contents] [Prev] [Next] [Index] [Report an Error]

# Setting Up SAE Communities (C-Web Interface)

You can configure the following for SAE communities:

- Define the members of an SAE community by adding the IP addresses of SAEs in the community to the virtual router object of the network device in the directory.

  See Creating Virtual Routers for the CMTS Device (C-Web Interface) .

- Specify the name of the community manager.

  See Configuring the SAE to Manage PCMM Devices (C-Web Interface).

- Configure parameters for the SAE community manager.

  See Configuring the SAE Community Manager with the C-Web Interface .

- If there is a firewall in the network, configure the firewall to allow SAE messages through.

#### Related Topics

- Setting Up SAE Communities with SRC CLI
- Using the SAE in a PCMM Environment

[Contents] [Prev] [Next] [Index] [Report an Error]