> - Downloads
> - Configuring the SAE to Manage JUNOSe Routers (C-Web Interface)
> - Related Topics
> - Configuring the SAE to Manage JUNOSe Routers with the CLI
> - Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices
> - Monitoring Interactions Between the SAE and the JUNOSe Router
> - Troubleshooting Problems with Managing JUNOSe Routers
> - COPS Connection Between JUNOSe Routers and the SAE

> # Configuring the SAE to Manage JUNOSe Routers (C-Web Interface)

> To set up the SAE to manage JUNOSe routers, configure a router driver that specifies a COPS server that can accept COPS connections from the COPS client in JUNOSe routers.

> To configure the SAE to manage JUNOSe routers:

> 1. Click Configure, expand Shared>SAE>Configuration>Driver, and then click JUNOSe.

>    The JUNOSe pane appears.

> 2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.