[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the IMS AAA Server

Tasks to set up the IMS AAA Server in the SRC network are:

- Configure the local elements for the IMS AAA Server.
  - Identification—IMS AAA Server
  - Diameter configuration—Transport port protocol
  - RADIUS configuration—AAA ports
- Configure the remote network elements.
  - The Diameter elements are for the C Series Controller and include: Origin host, IP address, port protocol, and function (SRC).
  - The RADIUS elements are for the NAS device and include: Name, IP address, and function.
- Review the custom router template for the NAS device. The service template element lists the parameters needed for service activation on the NAS device.

For information about configuring the IMS AAA Server with the IMS AAA Server Administrator, see the IMS AAA Server Administration Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]