> - Downloads
> - Before You Configure Redundancy for a Redirect Server
> - Related Topics
> - Configuring a Redundant Redirect Server (SRC CLI)
> - Configuring a Redundant Redirect Server (C-Web Interface)
> - Overview of Traffic Redirection
> - Redirect Server Redundancy

> # Before You Configure Redundancy for a Redirect Server

> If you plan to use a redundant configuration for the redirect server, ensure that:

> - If you use a next-hop address for policies that capture web traffic and send it to the redirect server, that the virtual IP address to be used is also the next-hop address.
> - The redirect server has SNMP write access to the virtual routers connected to it. Each VR must have at least a write community configured. (The static route from the virtual IP address to the server’s real IP address is installed on the router through SNMP.)
> - If additional access controls are enabled on the JUNOSe router, the hosts on which the redirect server runs must be included.

> #### Published: 2009-09-13

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.