> - Downloads
> - Defining a Congestion Point Profile (C-Web Interface)
> - Related Topics
> - Congestion Point Expressions
> - Classifying Interfaces (SRC CLI).
> - Configuring Congestion Point Classification (C-Web Interface)
> - Overview of Congestion Point Classification

> # Defining a Congestion Point Profile (C-Web Interface)

> You can create a congestion point profile that automatically performs congestion point classification. This profile supports only edge mode and dual mode for SRC ACP.

> To define a congestion point profile:

> 1. Click Configure>Shared>Congestion Points.

>    The Congestion Point Profile pane appears.

> 2. In the Create new list, select Profile. Type a name for the new profile in the dialog box, and click OK.

>    The Profile screen appears.

> 3. Enter information as described in the Help text in the main pane, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.