[Contents] [Prev] [Next] [Index] [Report an Error]

# Stopping the SRC Client on a JUNOSe Router

JUNOSe routers use an SRC client to interact with the SAE. See JUNOSe Broadband Access Configuration Guide for complete information about configuring the SRC client on the JUNOSe router.

To stop the SRC client:

1. Access the router CLI.

   See Accessing the Router CLI .

2. Access Global configuration mode.
   `
   host1#configure terminal
   `
3. Switch to the virtual router for which you want to stop an SRC client.
   `
   host1(config)#virtual-router <vrName>
   `
4. Disable the SRC client.
   `
   host1:<vrName>(config)#no sscc enable
   `

#### Related Topics

- Starting the SRC Client on a JUNOSe Router
- Viewing Statistics for All JUNOSe Device Drivers (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]