> - Downloads
> - Configuring the SAE for a Cable Network Environment (SRC CLI)
> - Related Topics
> - Overview of a PCMM Environment
> - Configuring the SAE for a Cable Network Environment (C-Web Interface)
> - Configuring the SAE to Manage PCMM Devices (C-Web Interface).
> - Configuring an SAE Group .

> # Configuring the SAE for a Cable Network Environment (SRC CLI)

> The tasks to configure the SAE for a cable network environment are:

> 1. Configure the SAE to manage PCMM devices.

>    Configuring the SAE to Manage PCMM Devices (SRC CLI).

> 2. Configure the session store.

>    See Configuring the Session Store Feature.

> 3. Set up SAE communities.

>    See Setting Up SAE Communities (SRC CLI).

> 4. (Optional) Configure SAE properties for the event notification API.

>    See Configuring SAE Properties for the Event Notification API (SRC CLI) (if you are using an external address manager).

> 5. (Optional) Configure record-keeping server peers for plug-ins.

>    See Configuring Record-Keeping Server Peers for Plug-Ins (SRC CLI) (if you are using the RKS plug-in).

> 6. (Optional) Configure PCMM record-keeping server plug-ins.

>    See Configuring PCMM Record-Keeping Server Plug-Ins (SRC CLI) (if you are using the SAE’s embedded policy server).

> 7. (Optional) Configure CMTS-specific RKS plug-ins.

>    See Configuring CMTS-Specific RKS Plug-Ins (SRC CLI).

> In addition to configuring the SAE, you need to:

> 1. Configure the CMTS device in the directory (if you are using the SAE’s embedded policy server).

>    See Adding Objects for CMTS Devices (SRC CLI) .

> 2. Configure the NIC (if you are using assigned IP subscribers).

>    See Using the NIC Resolver.

> 3. Enable the Common Open Policy Service (COPS) interface on the CMTS device. See the documentation for your CMTS device for information about how to do this.

> #### Published: 2009-09-23

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.