> - Downloads
> - Changing the Location of Data in the Directory
> - Related Topics
> - Configuring Initial Directory Eventing Properties for SRC Components
> - Configuring Basic Local Properties
> - Configuration Statements for Local Configuration
> - Managing Directory Communication

> # Changing the Location of Data in the Directory

> In most cases, you use the default configuration for the location of SRC data in the directory:

> - Administrator-defined configuration data—ou=staticConfiguration,ou=Configuration,o=Management,o=umc
> - Programmatically defined configuration data—ou=dynamicConfiguration,ou=Configuration,o=Management, o=umc

> You can specify the full distinguished name (DN), or a DN relative to a base DN, identified as <base>.

> You can change the location of data in the directory at the Expert CLI editing level.

> Use the following configuration statements to change the location of data for a component in the directory:

> `
> slot number component-name initial {
>   static-dn static-dn ;
>   dynamic-dn dynamic-dn ;
> }
> `

> To change the location of data in the directory:

> 1. From configuration mode, access the configuration statement that specifies the configuration for a component on a slot.
>    `
>    [edit]
>    user@host# edit slot number nic initial
>    `

>    For example:

>    `
>    [edit]
>    user@host# edit slot 0 nic initial
>    `
> 2. (Optional) Change the location of administrator-defined configuration data in the directory
>    `
>    [edit slot 0 nic initial]
>    user@host# set static-dn static-dn
>    `
> 3. (Optional) Change the location of programmatically defined configuration data in the directory.
>    `
>    [edit slot 0 nic initial]
>    user@host# set dynamic-dn dynamic-dn
>    `

> #### Published: 2009-09-25

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.