[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring CMTS-Specific RKS Plug-Ins (SRC CLI)

You can configure an RKS plug-in for specific CMTS devices. When there are events for the CMTS device, the SAE sends the events to the specified plug-in.

Use the following configuration statement to assign a CMTS-specific RKS plug-in.

`

shared sae configuration driver pcmm cmts-specific-rks-plug-ins name {
  rks-plug-in rks-plug-in ;
}

`

To configure a CMTS-specific RKS plug-in:

1. From configuration mode, access the configuration statements for RKS plug-ins. In this sample procedure, west-region is the name of the SAE group, and cmtsPlugin is the name of the plug-in assignment.
   `
   user@host# edit shared sae group west-region configuration driver pcmm cmts-specific-rks-plug-ins cmtsPlugin
   `
2. Specify the name of the CMTS-specific RKS plug-in.
   `
   [edit shared sae group west-region configuration driver pcmm cmts-specific-rks-plug-ins cmtsPlugin]
   user@host# set rks-plug-in rks-plug-in
   `
3. (Optional) Verify your configuration.

       [edit shared sae group west-region configuration driver pcmm cmts-specific-rks-plug-ins cmtsPlugin]
       user@host# show
       rks-plug-in rksPlugin;

#### Related Topics

- Configuring CMTS-Specific RKS Plug-Ins (C-Web Interface)
- Configuring Record-Keeping Server Peers for Plug-Ins (SRC CLI)
- Configuring PCMM Record-Keeping Server Plug-Ins (SRC CLI)
- Adding Objects for CMTS Devices (SRC CLI)
- Initially Configuring the SAE

[Contents] [Prev] [Next] [Index] [Report an Error]