[Contents] [Prev] [Next] [Index] [Report an Error]

# Specifying Initialization Scripts on the SAE

Use the following configuration statements to specify initialization scripts for third-party devices:

`

shared sae configuration driver scripts {
  extension-path extension-path ;
  general general ;
}

`

To configure initialization scripts for third-party devices:

1. From configuration mode, access the configuration statements that configure initialization scripts.
   `
   user@host# edit shared sae configuration driver scripts
   `
2. Specify the initialization script for third-party devices.
   `
   [edit shared sae configuration driver scripts]
   user@host# set general general
   `
3. Configure a path to scripts that are not in the default location, /opt/UMC/sae/lib.
   `
   [edit shared sae configuration driver scripts]
   user@host# set extension-path extension-path
   `
4. (Optional) Verify your initialization script configuration.

       [edit shared sae configuration driver scripts]
       user@host# show

#### Related Topics

- Specifying Initialization Scripts on the SAE
- Setting Up Script Services
- Copying Initialization Scripts to the C Series Controller
- Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices

[Contents] [Prev] [Next] [Index] [Report an Error]