[Contents] [Prev] [Next] [Index] [Report an Error]

# Adding Virtual Router Objects

Use the following configuration statements to add a virtual router:

`

shared network device name virtual-router name {
  sae-connection [ sae-connection ...];
  snmp-read-community snmp-read-community ;
  snmp-write-community snmp-write-community ;
  scope [ scope ...];
  tracking-plug-in [ tracking-plug-in ...];
}

`

To add a virtual router:

1. From configuration mode, access the configuration statements for virtual routers. You must specify the name of a device with lowercase characters. This sample procedure uses proxy_device as the name of the router object. For third-party devices, use the name default for the virtual router.
   `
   user@host# edit shared network device proxy_device virtual-router default
   `
2. Specify the addresses of SAEs that can manage this router. This step is required for the SAE to work with the router.
   `
   [edit shared network device proxy_device virtual-router default]
   user@host# set sae-connection [ sae-connection ...]
   `

   To specify the active SAE and the redundant SAE, enter an exclamation point (!) after the hostname or IP address of the connected SAE. For example:

   `
   [edit shared network device proxy_device virtual-router default]
   user@host# set sae-connection [sae1! sae2!]
   `
3. (Optional) Specify an SNMP community name for SNMP read-only operations for this virtual router.
   `
   [edit shared network device proxy_device virtual-router default]
   user@host# set snmp-read-community snmp-read-community
   `
4. (Optional) Specify an SNMP community name for SNMP write operations for this virtual router.
   `
   [edit shared network device proxy_device virtual-router default]
   user@host# set snmp-write-community snmp-write-community
   `
5. (Optional) Specify service scopes assigned to this virtual router. The scopes are available for subscribers connected to this virtual router for selecting customized versions of services.
   `
   [edit shared network device proxy_device virtual-router default]
   user@host# set scope [ scope ...]
   `
6. (Optional) Specify the plug-ins that track interfaces that the SAE manages on this virtual router.
   `
   [edit shared network device proxy_device virtual-router default]
   user@host# set tracking-plug-in [ tracking-plug-in ...]
   `
7. (Optional) Verify your configuration.

       [edit shared network device proxy_device virtual-router default]
       user@host# show
       sae-connection 10.8.221.45;
       snmp-read-community ********;
       snmp-write-community ********;
       scope POP-Toronto;
       tracking-plug-in flexRadius;

#### Related Topics

- Adding Objects for Network Devices (C-Web Interface)
- Adding Objects for Network Devices
- Overview of Integrating Network Devices into the SRC Network

[Contents] [Prev] [Next] [Index] [Report an Error]