[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing the Route Information

#### Purpose

You can use the traceroute command to get information about the hops between the local system and a remote host.

#### Action

To view route information:

`user@host> traceroute 192.2.7.48`

    traceroute to 192.2.7.48 (192.2.7.48), 30 hops max, 46 byte packets
     1  host (192.2.7.45)  3000.716 ms !H  3000.733 ms !H  3001.272 ms !H

For information about all the options for the traceroute command, see the SRC PE CLI Command Reference.

#### Related Topics

- Viewing Routing Table Information
- Viewing Interface Information
- Testing Connectivity to Remote Hosts
- Overview of Commands to Troubleshoot Connections to Remote Hosts

[Contents] [Prev] [Next] [Index] [Report an Error]