[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the Pseudo-RADIUS Server for External Subscriber Monitor

Use the following configuration statements to configure External Subscriber Monitor as a RADIUS accounting server:

`

slot number external-subscriber-monitor radius-accounting {
  port port;
  service-type (all | login | framed | callback-login | callback-framed | outbound | administrative | nas-prompt | authenticate-only | callback-nas-prompt | callback-check | callback-administrative);
  allow [allow...];
  deny [deny...];
  maximum-queue-length maximum-queue-length;
}

`

To configure the RADIUS accounting server:

1. From configuration mode, access the configuration statement that configures the RADIUS server.
   `
   user@host# edit slot 0 external-subscriber-monitor radius-accounting
   `
2. (Optional) Specify the listening port for RADIUS requests.
   `
   [edit slot 0 external-subscriber-monitor radius-accounting]
   user@host# set port port
   `
3. (Optional) Specify the service type of the RADIUS packets that will be forwarded.
   `
   [edit slot 0 external-subscriber-monitor radius-accounting]
   user@host# set service-type service-type
   `
4. (Optional) Specify a list that filters which packets are forwarded to the SAE based on NAS ID or NAS IP.
   `
   [edit slot 0 external-subscriber-monitor radius-accounting]
   user@host# set allow [allow...]
   `
5. (Optional) Specify a list that filters which packets are forwarded to the SAE based on NAS ID or NAS IP.
   `
   [edit slot 0 external-subscriber-monitor radius-accounting]
   user@host# set deny [deny... ]
   `
6. Specify the maximum number of unacknowledged RADIUS messages to be received from the RADIUS server before it discards new messages.
   `
   [edit slot 0 external-subscriber-monitor radius-accounting]
   user@host# set maximum-queue-length set maximum-queue-length
   `
7. (Optional) Verify your configuration.
   `
   [edit slot 0 external-subscriber-monitor radius-accounting]
   user@host# show
   `

#### Related Topics

- Configuring the Pseudo-RADIUS Server for External Subscriber Monitor (C-Web Interface)
- Configuring External Subscriber Monitor
- Configuring Event Notification for External Subscriber Monitor
- Configuring the NIC Proxy for the Pseudo-RADIUS Server
- Viewing Statistics for External Subscriber Monitor

[Contents] [Prev] [Next] [Index] [Report an Error]