[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the RADIUS Local IP Address and NAS ID with the C-Web Interface

To set the local RADIUS address and network access server (NAS ID):

1. Click Configure, and expand Slot.
2. Expand the slot for which you want to configure SAE, expand SAE, and then click Radius.

   The Slot SAE pane appears.

3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring the RADIUS Local IP Address and NAS ID (SRC CLI)
- Initially Configuring the SAE with the C-Web Interface
- Configuring Local Properties for the SAE with the C-Web Interface
- Configuring the Directory Location for SAE Data with the C-Web Interface

[Contents] [Prev] [Next] [Index] [Report an Error]