> - Downloads
> - Configuring Traffic-Shape Actions (SRC CLI)
> - Related Topics
> - Before You Configure SRC Policies
> - Configuring Traffic-Class Actions (SRC CLI)
> - Configuring Traffic-Mirror Actions (SRC CLI)
> - Configuring Traffic-Shape Actions (C-Web Interface)

> # Configuring Traffic-Shape Actions (SRC CLI)

> Traffic-shape actions specify the maximum rate of traffic transmitted on an interface. You can create traffic-shape actions in JUNOS shaping policy rules.

> The type of action that you can create depends on the type of policy rule. See Policy Information Model.

> Use the following configuration statements to configure traffic-shape actions:

> `
> policies group name list name rule name traffic-shape name {
>   rate rate ;
>   description description ;
> }
> `

> To configure a traffic-shape action:

> 1. From configuration mode, enter the traffic-shape configuration. For example, in this procedure, tsa is the name of the traffic-shape action.
>    `
>    user@host# edit policies group junos list trafficShaping rule shaping traffic-shape tsa
>    `
> 2. (Optional) Configure the maximum transmission rate.
>    `
>    [edit policies group junos list trafficShaping rule shaping traffic-shape tsa]
>    user@host# set rate rate
>    `
> 3. (Optional) Enter a description for the traffic-shape action.
>    `
>    [edit policies group junos list trafficShaping rule shaping traffic-shape tsa]
>    user@host# set description description
>    `
> 4. (Optional) Verify the traffic-shape action configuration.

>        [edit policies group junos list trafficShaping rule shaping traffic-shape tsa]
>        user@host# show
>        rate 10200000;
>        description "Traffic-shaping action";

> #### Published: 2009-09-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.