[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the RADIUS Local IP Address and NAS ID (SRC CLI)

Use the following configuration statements to set the local RADIUS address and network access server (NAS ID):

`

slot number sae radius {
  local-address local-address ;
  local-nas-id local-nas-id ;
}

`

To set the local RADIUS address and NAS ID:

1. From configuration mode, access the SAE RADIUS configuration. This configuration is under the slot 0 hierarchy.
   `
   [edit]
   user@host# edit slot 0 sae radius
   `
2. Configure the local IP address that the SAE uses to communicate with RADIUS servers.
   `
   [edit slot 0 sae radius]
   user@host# set local-address local-address
   `
3. Configure the NAS ID that identifies the SAE when it sends RADIUS authentication and accounting records. Typically, the NAS ID is the name of the SAE host.
   `
   [edit slot 0 sae radius]
   user@host# set local-nas-id local-nas-id
   `
4. (Optional) Verify your configuration.

       [edit slot 0 sae radius]
       user@host# show
       local-address 10.10.4.20;
       local-nas-id SAE.host1;

#### Related Topics

- Configuring the RADIUS Local IP Address and NAS ID with the C-Web Interface
- Configuring Local Properties for the SAE (SRC CLI)
- Configuring an SAE Group
- Initially Configuring the SAE
- Creating Grouped Configurations for the SAE (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]