> - Downloads
> - Modifying the Subscriber Configuration (C-Web Interface)
> - Related Topics
> - Modifying the Subscriber Configuration
> - Modifying the JPS Configuration (C-Web Interface)
> - Configuring Subscriber IP Pools as IP Address Ranges (C-Web Interface)
> - Configuring Subscriber IP Pools as IP Subnets (C-Web Interface)

> # Modifying the Subscriber Configuration (C-Web Interface)

> To locate the CMTS device associated with a subscriber, the JPS maps the subscriber IP address in a message to the CMTS IP address to which the message must be delivered. This mapping specifies the subscriber IP pools associated with CMTS devices.

> The tasks to configure a CMTS device to which the JPS can connect and the pools of subscriber IP addresses that are managed by that CMTS device are:

> 1. Configuring Subscriber IP Pools as IP Address Ranges (C-Web Interface)
> 2. Configuring Subscriber IP Pools as IP Subnets (C-Web Interface)

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.