> - Downloads
> - Configuring RADIUS and TACACS+ Authentication on a C Series Controller
> - Related Topics
> - Configuring RADIUS and TACACS+ Authentication on a C Series Controller (C-Web Interface)
> - Configuring TACACS+ Authentication (C-Web Interface)
> - Removing an SRC Authentication Method from the Authentication Order
> - Example: Configuring SRC Authentication

> # Configuring RADIUS and TACACS+ Authentication on a C Series Controller

> The SRC software always performs password authentication on a C Series Controller. You can configure RADIUS or TACACS+ (or both) authentication to complement password authentication. In this case, the software performs RADIUS or TACACS+ (or both) authentication before password authentication.

> To configure RADIUS and TACACS+ authentication for users who access a C Series Controller:

> 1. Configure the connection to the RADIUS or TACACS+ server.

>    See Configuring RADIUS Authentication (SRC CLI).

> 2. Configure the authentication order.

>    See A C Series Controller as a RADIUS Client and TACACS+ Client .

> 3. Configure template accounts.
> 4. (Optional) Configure individual user profiles.

>    See Overview of SRC User Accounts.

> #### Published: 2009-09-25

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.