[Contents] [Prev] [Next] [Index] [Report an Error]

## DHCP Options Supported on the SAE

Table 7 lists the DHCP options are available.

Table 7: DHCP Options Supported on the SAE

Option Name | Option Number | Option Type
--- | --- | ---
subnet-mask | 1 | ip-address
time-offset | 2 | int32
routers | 3 | ip-address
time-servers | 4 | ip-address
ien116-name-servers | 5 | ip-address
domain-name-servers | 6 | ip-address
log-servers | 7 | ip-address
cookie-servers | 8 | ip-address
lpr-servers | 9 | ip-address
impress-servers | 10 | ip-address
resource-location-servers | 11 | ip-address
host-name | 12 | string
boot-size | 13 | int16
merit-dump | 14 | string
domain-name | 15 | string
swap-server | 16 | ip-address
root-path | 17 | string
extension-path | 18 | string
ip-forwarding | 19 | int8
non-local-source-routing | 20 | int8
policy-filter | 21 | ip-address
max-dgram-reassembly | 22 | int16
default-ip-ttl | 23 | int8
path-mtu-aging-timeout | 24 | int32
path-mtu-plateau-table | 25 | int16
interface-mtu | 26 | int16
all-subnets-local | 27 | int8
broadcast-address | 28 | ip-address
perform-mask-discovery | 29 | int8
mask-supplier | 30 | int8
router-discovery | 31 | int8
router-solicitation-address | 32 | ip-address
static-routes | 33 | ip-address
trailer-encapsulation | 34 | int8
arp-cache-timeout | 35 | int32
ieee802-3-encapsulation | 36 | int8
default-tcp-ttl | 37 | int8
tcp-keepalive-interval | 38 | int32
tcp-keepalive-garbage | 39 | int8
nis-domain | 40 | string
nis-servers | 41 | ip-address
ntp-servers | 42 | ip-address
netbios-name-servers | 44 | ip-address
netbios-dd-server | 45 | ip-address
netbios-node-type | 46 | int8
netbios-scope | 47 | string
font-servers | 48 | ip-address
x-display-manager | 49 | ip-address
requested-ip-address | 50 | ip-address
ip-address-lease-time | 51 | int32
option-overload | 52 | int8
dhcp-msg-type | 53 | int8
server-identifier | 54 | ip-address
parameter-request-list | 55 | data-string
message | 56 | string
maximum-dhcp-msg-size | 57 | int16
renewal-time | 58 | int32
rebinding-time | 59 | int32
vendor-class-identifier | 60 | data-string
client-identifier | 61 | data-string
nisplus-domain | 64 | string
nisplus-servers | 65 | ip-address
tftp-server-name | 66 | string
bootfile-name | 67 | string
mobile-ip-home-agent | 68 | ip-address
smtp-server | 69 | ip-address
pop-server | 70 | ip-address
nntp-server | 71 | ip-address
www-server | 72 | ip-address
finger-server | 73 | ip-address
irc-server | 74 | ip-address
streettalk-server | 75 | ip-address
streetalk-directory-assistance-server | 76 | ip-address

#### Related Topics

- Selecting DHCP Parameters
- Classifying DHCP Subscribers (SRC CLI)
- Creating DHCP Profiles (SRC CLI)
- Sending DHCP Options to the JUNOSe Router
- Syntax for DHCP Classification Targets
- DHCP Classification Conditions

[Contents] [Prev] [Next] [Index] [Report an Error]