[Contents] [Prev] [Next] [Index] [Report an Error]

# Defining an Alarm for an SNMP Monitor That Compares Values Against Thresholds (SRC CLI)

You can configure a monitor to compare a sample value for a MIB object to a threshold encountered as the value rises and a threshold encountered as the value falls.

| Note: Configure only one monitor test at a time.

Before you define an alarm type, configure the associated SNMP alarm.

See Configuring an SNMP Alarm on a C Series Controller (SRC CLI).

To configure an alarm for a monitor that compares a sample value to an upper threshold value and a lower threshold value:

1. Define the upper threshold against which to compare a rising sample value. For example:
   `
   [edit snmp monitor alarm thresholds threshold-test]
   user@host# set rising-threshold 2
   `
2. Define the lower threshold against which to compare a falling sample value. For example:
   `
   [edit snmp monitor alarm threshold-alarm]
   user@host# set falling-threshold 1
   `

#### Related Topics

- Defining an Alarm for an SNMP Monitor That Compares Object Values (SRC CLI)
- Defining an Alarm to Monitor the Status of an Object (SRC CLI)
- Configuring an SNMP Alarm on a C Series Controller (SRC CLI)
- Configuration Statements for Customized SRC SNMP Monitors
- SNMP Monitoring on C Series Controllers

[Contents] [Prev] [Next] [Index] [Report an Error]