[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the Directory Location for SAE Data with the C-Web Interface

You can configure the locations for dynamic and static configuration data in the directory.

To configure the directory location for configuration data:

1. Click Configure, and expand Slot.
2. Expand the slot for which you want to configure SAE, expand SAE, and then click Initial.

   The Initial pane appears.

3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Initially Configuring the SAE with the C-Web Interface
- Configuring Local Properties for the SAE with the C-Web Interface
- Configuring the RADIUS Local IP Address and NAS ID with the C-Web Interface

[Contents] [Prev] [Next] [Index] [Report an Error]